Water Test from Various Sources

Source
Testing for	Zephyrhills Bottled Spring Water
(A2)	Kirkland Bottled Water (A3)	Aquafina Bottled Water (A4)	FIJI
Bottled Water (A5)	Publix Bottled Spring Water
(A6)	Pure Life
Bottled Water (A7)	Coral Spring Improvement District
(A8)	Suggested Municipal Range	
pH	7.62	6.98	5.30	7.05	5.79	6.60	8.50	6.5-8.5	
Total Alkalinity
mg/L	163	18.0	2.00	139	ND	101	40	20-60 ppm	
Total Hardness
mg/L	179	0.54	ND	103	12.3	134	42.9	20-60 ppm	
Turbidity
(NTU)	0.05	0.15	0.15	0.25	0.10	0.15	0.20	< 0.3 NTU	
Color(CU)	5.0	5.0	5.0	5.0	5.0	5.0	5.0	< 15	
Total Chlorine Residual
(disinfection)	ND	ND	ND	ND	ND	ND	3.20	1.0-4.0 ppm	
Iron Content
mg/L	ND	ND	ND	ND	ND	0.0043	0.0095	< 0.3 ppm	

PPM - Parts per million. (1ppm = 1mg/L) - milligrams per liter.
ND - Analyte NOT DETECTED at or above the detection limit.
NTU – The standard unit used to measure the clarity, cloudiness, or haziness of liquids (turbidity) caused by suspended particles.
4/14/2026